For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the right front tire/wheel assembly. Refer to Tire and Wheel Removal and Installation .
2. Place drain pans under the vehicle as needed.

1 | Power Steering Fluid Reservoir Outlet Hose Clamp
2 | Power Steering Fluid Reservoir Outlet Hose
3 | Power Steering Pump Inlet Pipe Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten Tighten to 8 N·m (71 lb in).
4 | Power Steering Pump Inlet Pipe Seal Tip Discard the O-ring seal and use a NEW O-ring seal prior to installation.
5 | Power Steering Pump Inlet Pipe

#### Procedure

Fill and bleed the power steering system. Refer to Power Steering System Bleeding .

Tip
Clean any excess power steering fluid from the vehicle.