For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement.
2. Remove the RH defogger duct screws from the I/P upper trim panel.
3. Remove the RH defogger duct from the I/P upper trim panel.

### Installation Procedure

1. Inspect the seals, and replace if damaged, using Kent Industries adhesive backed foam tape P/N 46485 or equivalent.
2. Install the RH defogger duct to the I/P upper trim panel.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the RH defogger duct screws to the I/P upper trim panel.

Tighten the screws to 1 N·m (9 lb in).

4. Install the instrument panel (I/P) upper trim panel. Refer to Instrument Panel Upper Trim Panel Replacement.