For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat inner recliner cover. Refer to Rear Seat Back Recliner Cover Replacement .
2. Remove the rear seat outer recliner cover. Refer to Rear Seat Back Recliner Cover Replacement .
3. Remove the rear seat latch covers.

1 | Rear Seat No. 1 Seat Cushion Cover

#### Procedure

1. Disconnect the seat cover j-channel from the seat frame.
2. Remove the seat cushion cover and pad as an assembly from the seat cushion frame.

2 | Rear Seat No. 1 Seat Cushion Pad (60 percent seat shown, 40 percent seat similar) Tip Remove the seat cushion pad from the seat cushion cover.