For 1990-2009 cars

Table 1: | Pump Assembly Installation
Table 2: | Transfer Drive Gear Assembly Installation

### Pump Assembly Installation

Callout | Component Name
--- | ---
1 | Driven Sprocket Thrust Washer
2 | Drive Sprocket Thrust Washer
3 | Install Drive Link Assembly Tip Install as an assembly.
4 | A/Trans Fluid Pump Assembly Tip Rotating the drive sprocket and link assembly while installing the oil pump will aid in aligning the driven sprocket and oil pump drive shaft splines.
5 | A/Trans Fluid Pump Bolt M6 x 25 (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure:

Tighten in sequence shown.

Tighten
12 N·m (106 lb in).

### Transfer Drive Gear Assembly Installation

Callout | Component Name
--- | ---
1 | Drive Sprocket Thrust Washer
2 | Front Differential Transfer Drive Gear Support Assembly
3 | Front Differential Transfer Drive Gear Support Bolt M8 x 25 (Qty: 9) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Tighten in sequence shown.

Tighten
10 N·m (89 lb in) plus 50 degrees ± 4 degrees.

#### Special Tools:

J 45059 Angle Meter

For equivalent regional tools, refer to Special Tools.

4 | Front Differential Carrier Baffle
5 | Front Differential Carrier Baffle Bolt M6 x 25 Tighten 12 N·m (106 lb in).