For 1990-2009 cars

## Front Lower Control Arm Bushing Replacement Rear Bushing

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
3. Remove the lower control arm. Refer to Lower Control Arm Replacement .
4. Remove the rear bushing nut.
5. Remove the rear bushing.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear bushing to the lower control arm.

Tighten
Tighten the nut to 150 N·m (110 lb ft).

2. Install the lower control arm. Refer to Lower Control Arm Replacement .
3. Install the front tire and wheel assembly. Refer to Tire and Wheel Removal and Installation .
4. Lower the vehicle.