For 1990-2009 cars

1. Install a NEW oil suction tube seal onto the oil suction tube. DO NOT reuse the old oil suction tube seal.
2. Install the oil suction pipe.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the oil suction pipe bolts.

Tighten
Tighten the oil suction pipe bolts to 10 N·m (89 lb in).

4. Install the oil pan scraper.
5. Install the oil pan scraper bolts.

Tighten
Tighten the oil pan scraper bolts to 10 N·m (89 lb in).

6. Install the oil pan drain plug and NEW O-ring seal.

Tighten
Tighten the oil pan drain plug to 20 N·m (15 lb ft).