For 1990-2009 cars

### Removal Procedure

1. Remove the front brake rotor. Refer to Front Brake Rotor Replacement.
2. Disconnect the wheel speed sensor electrical connector, if equipped.
3. Remove the wheel speed sensor electrical connector from the connector bracket.
4. Remove the front wheel drive shaft spindle nut.
5. Remove the speed sensor. Refer to Front Wheel Speed Sensor Replacement.
6. Support the wheel drive shaft with heavy mechanic's wire or equivalent.
7. Remove and discard the wheel bearing/hub mounting bolts.
8. Remove the wheel bearing/hub assembly from the steering knuckle.

### Installation Procedure

1. Install the wheel bearing/hub assembly to the steering knuckle.
2. Clean the threads of the bolts with the proper cleaner.

Important: Allow the threadlocker to set for 10 minutes before using.

3. Apply threadlocker GM P/N 89021297 (Canadian P/N 10953488) on 2/3 of the bolts threads.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the wheel bearing/hub mounting bolts.

Tighten
Tighten the bolts to 130 N·m (96 lb ft).

5. Install the wheel drive shaft spindle nut.

Tighten
Tighten the nut to 205 N·m (151 lb ft).

6. Install the wheel speed sensor electrical connector to the mounting bracket, if equipped.
7. Connect the wheel speed sensor electrical connector.
8. Install the speed sensor. Refer to Front Wheel Speed Sensor Replacement.
9. Install the front brake rotor. Refer to Front Brake Rotor Replacement.