For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Wiper Arm Nut Finish Cap
2 | Rear Wiper Arm Nut Caution: Refer to Fastener Caution in the Preface section. Tip Hold the blade tip on the first defroster grid line while torquing the wiper arm nut. Tighten
10 N·m (89 lb in)

3 | Windshield Washer Arm Assembly Tip

• | Position wiper blade assembly above the blackout strip as shown in the illustration.

• | Position the blade element on the first defroster grid line, above the blackout.

• | Secure the nut.

• | Install the rear wiper arm nut finish cap.

• | Operate the windshield wipers and inspect for proper operation.