For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the cooling fan and shroud. Refer to Cooling Fan and Shroud Replacement
3. Disconnect the high pressure switch electrical connector.

1 | Compressor Hose Assembly Nut (Qty: 2). Notice: Refer to Fastener Notice in the Preface section. Tighten 20 N·m (15 lb ft)
2 | A/C Compressor Assembly Hose

#### Procedure

Remove and discard the sealing washer. Refer to Sealing Washer Replacement .