For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove upper extension trim panel. Refer to Upper Extension Trim Panel Replacement .
2. Remove door handle bezel. Refer to Door Handle Bezel Replacement .

1 | Front Side Door Trim Panel Plug
2 | Front Side Door Trim Panel Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2.5 N·m (22 lb in)
3 | Front Side Door Trim Panel Assembly
4 | Front Side Door Trim Panel Retainer (Qty: 11)