For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Inflator Module Handling and Storage Warning in the Preface section.

#### Preliminary Procedures

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove center pillar lower molding. Refer to Center Pillar Lower Garnish Molding Replacement.
3. Release seat belt from seat side anchor.

1 | Seat Belt Retractor Pretensioner Adjuster Cover
2 | Seat Belt Retractor Pretensioner Bolt Caution: Refer to Fastener Caution in the Preface section. Tip Apply GM P/N 12345382 (Canadian P/N 10953489), Permatex® 24200 or equivalent on all restraint fasteners prior to installation. Tighten
45 N·m (33 lb ft)

3 | Seat Belt Retractor Pretensioner Adjuster Bolt Tighten 45 N·m (33 lb ft)
4 | Seat Belt Retractor Pretensioner Assembly

#### Procedure

1. Disconnect the electrical connectors.
2. Discharge and dispose of pretensioner assembly using the appropriate procedure. Refer to Pretensioner Handling and Scrapping.