For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left side instrument panel sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side .
2. Remove the left side knee bolster. Refer to Knee Bolster Replacement .

1 | Brake Pedal Position Sensor Bolt Tip

• | Calibrate the position sensor. Refer to Brake Pedal Position Sensor Calibration .

• | Do not reuse the position sensor or bolt. Always use a new sensor and bolt.

2 | Brake Pedal Position Sensor Assembly Caution: Refer to Fastener Caution in the Preface section. Tip Disconnect the electrical connector. Tighten
2.5 N·m (22 lb in)