For 1990-2009 cars

### Removal Procedure

1. Remove the powertrain control module (PCM) (2) from the battery box cover (1) and relocate to the side.
2. Release the locking tab (1) on the side of the battery box.
3. Release the alignment tabs (2) on the front of the battery box.
4. Remove the battery box lid (3).
5. Disconnect the positive and negative battery cables. Refer to Battery Negative Cable Disconnection and Connection .
6. Remove the battery hold down bolt (5), battery hold down (4), and washer (3).
7. Remove the battery (1).

### Installation Procedure

1. Position the battery (1) in the battery box (2).
2. Install the washer (3) and battery hold down (4).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the hold down bolt (5).

Tighten
Tighten the hold down bolt to 15 N·m (11 lb ft).

4. Install the positive and negative battery cables. Refer to Battery Negative Cable Disconnection and Connection .
5. Position the battery lid (3) so that the alignment tabs (2) are in position.
6. Lock the locking tabs (1) on the side of the battery box.
7. Install the PCM (2) on the battery box cover (1).