For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank. Refer to Fuel Tank Replacement.
2. Disconnect the fuel pump module harness electrical connector from the fuel tank pressure sensor.
3. Position 2 flat-bladed screwdrivers, one on each side of the sensor, near the vacuum port.
4. Carefully use the screwdrivers to lift and release the sensor from the fuel pump module.

### Installation Procedure

1. Install the fuel tank pressure sensor to the fuel pump module assembly. Ensure that the sensor grommet is fully seated to the pump module.
2. Connect the pump module electrical connector to the fuel tank pressure sensor.
3. Install the fuel tank. Refer to Fuel Tank Replacement.