For 1990-2009 cars

### Removal Procedure

1. Remove the underhood electrical center bracket. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .
2. Disconnect the brake fluid level indicator switch electrical connector.
3. While simultaneously depressing the retaining tabs on the opposite side of the switch electrical connection, carefully pull the switch from the master cylinder reservoir.
4. Remove the low brake fluid level sensor.

### Installation Procedure

1. While noting the proper orientation, install the brake fluid level indicator switch to the master cylinder.
2. Press the brake fluid level indicator switch firmly into the master cylinder reservoir, ensuring that the retaining tabs are fully engaged.
3. Connect the brake fluid level indicator switch electrical connector.
4. Install the underhood electrical center bracket. Refer to Underhood Electrical Center or Junction Block Bracket Replacement .