For 1990-2009 cars

### Removal Procedure

Caution: In order to prevent SIR deployment, personal injury, or unnecessary SIR system repairs, do not strike the door or the door pillar in the area of the side impact sensor (SIS). Turn OFF the ignition and remove the key when performing service in the area of the SIS.

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door lower speaker. Refer to Radio Front Side Door Speaker Replacement .
3. Remove the check link bolts at the hinge pillar.
4. Remove the check link nuts from the door frame.
5. Remove the check link from the door through the speaker opening.

### Installation Procedure

1. Install the check link to the door frame.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts to the check link.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Install the check link bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install the front door lower speaker. Refer to Radio Front Side Door Speaker Replacement .
5. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .