For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove the wiper arm blade. Refer to Windshield Wiper Blade Replacement .

1 | Blade, Windshield Wiper Arm
2 | Bear Claws, Wiper Arm Blade
3 | Insert, Wiper Arm Blade Tip

1. Hold the wiper arm blade firmly and pull blade element from blade bear claws.
2. Passenger and driver side inserts are not interchangeable.