For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the steering column. Refer to Steering Column Replacement .
2. Remove the instrument panel retainer. Refer to Instrument Panel Retainer Replacement .
3. Remove the center air outlet duct. Refer to Center Air Outlet Duct Replacement .
4. Remove the windshield defroster duct. Refer to Windshield Defroster Duct Replacement .

1 | Instrument Panel Tie Bar to HVAC Module Assembly Nut (Qty: 3) Tip The nut on the lower left side is driven from front of vehicle rearward. Notice: Refer to Fastener Notice in the Preface section. Tighten
4 N·m (36 lb in)

2 | Instrument Panel Tie Bar to HVAC Module Assembly Bolt (Qty: 3) Tighten 4 N·m (36 lb in)
3 | Instrument Panel Tie Bar to HVAC Module Assembly Nut (Qty: 2) Tighten 4 N·m (36 lb in)
4 | Instrument Panel Tie Bar Nut (Qty: 6) Tighten 9 N·m (80 lb in)
5 | Instrument Panel Tie Bar Bolt (Qty: 6) Tighten 25 N·m (18 lb ft)
6 | Instrument Panel Tie Bar Assembly

#### Procedures

1. Note location and routing of the instrument panel wiring harness and ground straps prior to removal to ensure proper reinstallation.
2. Disconnect the instrument panel wiring harness and ground straps from the tie bar assembly.
3. With the aid of an assistant, lift the tie bar assembly straight up and then rearward removing the tie bar assembly from the vehicle.