For 1990-2009 cars

## Upper Extension Trim Panel Replacement Front Side Door

Callout | Component Name
--- | ---
1 | Front Side Door Upper Trim Panel Retainer (Qty: 1)
2 | Front Side Door Upper Trim Panel Assembly

#### Procedures

1. Pull on the top end of extension panel to disengage attaching clip.
2. Lift extension panel out from behind the door trim panel.
3. Use care to ensure sound deadener is in correct position when installing trim to door.
4. Disconnect electrical connectors.