For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the left rear trim panel. Refer to Quarter Lower Rear Trim Panel Replacement .
2. Remove the 3 auxiliary HVAC module mounting bolts. Refer to Auxiliary HVAC Module Replacement .
3. Reposition the auxiliary HVAC module inward to gain access to the temperature actuator.
4. Calibrate the actuators. Refer to Actuator Recalibration .

1 | Auxiliary Temperature Actuator Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Auxiliary Temperature Actuator Tip

• | The temperature actuator is mounted on the outboard side of the module.

• | Disconnect the electrical connector.