For 1990-2009 cars

### Removal Procedure

1. Remove the front seats. Refer to Front Seat Replacement - Bucket.
2. Remove the floor console. Refer to Console Replacement.
3. Partially remove the floor carpet from the front footwells to the B-pillars.
4. Remove the rear floor air outlet push pins from the floor pan.
5. Remove the rear floor air outlet from the floor pan.

### Installation Procedure

1. Install the rear floor air outlet to the floor pan.
2. Install the rear floor air outlet push pins to the floor pan.
3. Install the floor carpet to the B-pillars and the front footwells .
4. Install the floor console. Refer to Console Replacement.
5. Install the front seats. Refer to Front Seat Replacement - Bucket.