For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Remove the headlamp assembly. Refer to Headlamp Replacement .

1 | Side Marker Lamp Bulb Socket Tip Turn the lamp socket a quarter turn counter-clockwise in order to remove the socket from the headlamp assembly.
2 | Side Marker Lamp Bulb Tip Pull the marker lamp bulb straight from the socket.