For 1990-2009 cars

#### Front Seats

Front floor bucket seats are equipped with adjustable head restraints that can be released by the tab located at the base of the restraint. All models offer 2-way adjustment.

All models offer 4-way manual seat adjustment on the driver side and 2-way manual adjustment on the passenger side, as well as a manual recliner on each side. All seats offer the towel-bar control for forward/backward adjustment as well as a driver seat height adjuster lever which is located on the outer side panel. To operate the height adjuster, ratchet upward on the lever to raise the seat cushion and ratchet downward on the lever to lower the seat cushion. The recliner is operated by a lever on the lower outboard side of the front seat back.

#### Rear Seats

All vehicles have rear seat backs that fold forward using a latch lever located at the top of each seat back. Each seat back may be placed in an upright position or may be slightly reclined.

To fold the seat forward, pull upward on the latch and fold the seat forward. Pull on the latch to put the seat back in the up position. To recline the seatback, pull on the latch again while applying pressure to the rear seat back cushion. Pull again on the latch to put the seat back in the full-up position.