For 1990-2009 cars

### Removal Procedure

Note: Do not remove the drive belt from the vehicle entirely. Only slip it off the power steering pump and set it aside in the engine compartment.

1. Remove the drive belt. Refer to Drive Belt Replacement.
2. Remove as much power steering fluid from the remote power steering fluid reservoir as possible.
3. Remove the right side engine splash shield. Refer to Engine Splash Shield Replacement - Right Side.
4. Place drain pans under the vehicle as needed.
5. Compress the power steering reservoir outlet hose clamp (1) and disconnect the power steering reservoir outlet hose (2) from the power steering pump.
6. Disconnect the power steering gear inlet hose (1) from the power steering pump.
7. Remove the power steering pump bolts (1).
8. Remove the power steering pump through the right wheel house area.
9. Transfer the power steering pulley if needed. Refer to Power Steering Pump Pulley Replacement.

### Installation Procedure

1. Position the power steering pump to the vehicle through the right wheel house area.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the power steering pump bolts (1).

Tighten
Tighten to 50 N·m (37 lb ft).

3. Connect the power steering gear inlet hose (1) to the power steering pump.

Tighten
Tighten to 25 N·m (18 lb ft).

4. Compress the power steering reservoir outlet hose clamp (1) and connect the power steering reservoir outlet hose (2) to the power steering pump.
5. Install the right side engine splash shield. Refer to Engine Splash Shield Replacement - Right Side.
6. Clean any excess power steering fluid from the vehicle and remove the drain pans.
7. Install the drive belt. Refer to Drive Belt Replacement.
8. Fill and bleed the power steering system. Refer to Power Steering System Bleeding.