For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement .
2. Remove the sixty percent rear seat back cover and pad. Refer to Rear Seat Back Cushion Cover and Pad Replacement .

1 | Center Rear Seat Belt Retractor To Seat Bolt Notice: Refer to Fastener Notice in the Preface section. Tip Apply GM P/N 12345382 (Canadian P/N 10953489), Permatex® 24200 or equivalent on all seat belt fasteners prior to installation. Tighten
45 N·m (33 lb ft)

2 | Center Rear Seat Belt Retractor To Seat Nut Tip Apply GM P/N 12345382 (Canadian P/N 10953489), Permatex® 24200 or equivalent on all seat belt fasteners prior to installation. Tighten 45 N·m (33 lb ft)
3 | Center Rear Seat Belt Retractor Tip Make sure alignment slots are aligned correctly on reinstallation.