For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Turn Lamp Bulb Socket
2 | Turn Lamp Bulb Tip Pull the turn lamp bulb straight from the lamp socket.
3 | Caution: Refer to Halogen Bulb Caution in the Preface section. Headlamp Bulb (Hi/Lo)
4 | Park Auxiliary Bulb Socket
5 | Park Auxiliary Bulb Tip Pull the park auxiliary bulb straight from the lamp socket.
6 | Side Marker Lamp Bulb Socket
7 | Side Marker Lamp Bulb Tip Pull the side marker lamp bulb straight from the lamp socket.