For 1990-2009 cars

Connector 1: | Fuse Block - Underhood C1
Connector 2: | Fuse Block - Underhood C2
Connector 3: | Fuse Block - Underhood C3
Connector 4: | Fuse Block - I/P C1
Connector 5: | Fuse Block - I/P C2
Connector 6: | Fuse Block - I/P C3

### Fuse Block - Underhood C1

#### Connector Part Information

- OEM: 6098-5227
- Service: 88988708
- Description: 47-Way F LIF Series (WH)

#### Terminal Part Information

- Pins: 46
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 24, 24
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 5, 6, 7, 8, 9, 15, 16, 18, 19, 20, 26, 28, 29, 31, 32, 39, 40, 42, 27, 30
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins 5, 6, 7, 8, 9, 15, 16, 18, 19, 20, 26, 28, 29, 31, 32, 39, 40, 42 - E/C
- Core/Insulation Crimp: Pins 27, 30 - C/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 13, 23, 14, 25
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins 13, 23 - E/A
- Core/Insulation Crimp: Pins 14, 25 - 2/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Fuse Block - Underhood C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-4 | -- | -- | Not Used
5 | YE | 447 | Starter Relay Coil Control
6 | BK/WH | 451 | Ground
7 | PK | 439 | Ignition 1 Voltage
8 | D-GN | 59 | A/C Compressor Clutch Supply Voltage
9 | PK/BK | 5294 | Powertrain Main Relay Fused Supply (5)
10-12 | -- | -- | Not Used
13 | PK | 1339 | Ignition 1 Voltage
14 | PK/BK | 5291 | Ignition 1 Voltage
15 | D-BU | 473 | High Speed Cooling Fan Relay Control
16 | TN | 2759 | Low Reference
17 | -- | -- | Not Used
18 | D-GN/WH | 459 | A/C Compressor Clutch Relay Control
19 | PK/BK | 5294 | Powertrain Main Relay Fused Supply (5)
20 | PK | 1039 | Ignition 1 Voltage
21-22 | -- | -- | Not Used
23 | BN/WH | 419 | MIL Control
24 | PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)
PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)
25 | PK/BK | 5292 | Ignition 1 Voltage
26 | D-GN/WH | 465 | Fuel Pump Relay Control [- Primary]
27 | WH | 1310 | EVAP Canister Vent Solenoid Control
28 | WH | 17 | Stop Lamp Switch Signal
29 | BN | 4 | Accessory Voltage
30 | PK/BK | 5290 | Ignition 1 Voltage
31 | RD/WH | 1540 | Battery Positive Voltage
32 | BN | 5069 | Engine Main Relay Coil Control
33-38 | -- | -- | Not Used
39 | D-GN | 335 | Low Speed Cooling Fan Relay Control
40 | BN | 4 | Accessory Voltage
41 | -- | -- | Not Used
42 | RD/WH | 540 | Battery Positive Voltage
43-45 | -- | -- | Not Used
46 | PU | 6 | Starter Solenoid Crank Voltage
47 | -- | -- | Not Used

### Fuse Block - Underhood C2

#### Connector Part Information

- OEM: 6098-5229
- Service: 88988710
- Description: 50-Way F LIF Series (BK)

#### Terminal Part Information

- Pins: 1, 2, 34, 35
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 3, 11, 11, 12, 13, 22, 25, B, 14, 23, 24, 33, A
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins 3, 11, 11, 12, 13, 22, 25, B - E/A
- Core/Insulation Crimp: Pins 14, 23, 24, 33, A - 2/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 4, 6, 7, 8, 9, 15, 17, 18, 19, 20, 21, 27, 28, 29, 30, 31, 32, 36, 36, 38, 39, 40, 41, 41, 42, 5, 10, 16
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins 4, 6, 7, 8, 9, 15, 17, 18, 19, 20, 21, 27, 28, 29, 30, 31, 32, 36, 36, 38, 39, 40, 41, 41, 42 - E/C
- Core/Insulation Crimp: Pins 5, 10, 16 - C/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 43, 46, 47, 44, C
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: Pins 43, 46, 47 - D/G
- Core/Insulation Crimp: Pins 44, C - A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Fuse Block - Underhood C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/WH | 140 | Battery Positive Voltage
2 | RD/BK | 742 | Battery Positive Voltage
3 | D-GN | 1619 | Trailer Right Rear Turn/Stop Lamp Supply Voltage (V92)
4 | BN | 2109 | Trailer Park Lamps Supply Voltage (V92)
5 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
6 | WH | 1080 | Park Lamp Relay Control
7 | PK/BK | 109 | Hood Ajar Switch Signal (AP3)
8 | TN/WH | 1969 | Headlamp High Beam Relay Control
9 | PU | 5531 | Hood Closed Switch Signal (AP3)
10 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
11 | L-BU | 20 | Stop Lamp Supply Voltage
L-BU | 20 | Stop Lamp Supply Voltage
12 | BN/WH | 309 | Right Park Lamp Supply Voltage
13 | YE | 1618 | Trailer Left Rear Turn/Stop Lamp Supply Voltage (V92)
14 | GY | 120 | Fuel Pump Supply Voltage
15 | L-BU | 1320 | CHMSL Supply Voltage
16 | RD/WH | 1740 | Battery Positive Voltage (MH6)
17 | RD/WH | 2440 | Battery Positive Voltage
18 | PK/WH | 1970 | Headlamp Low Beam Relay Control
19 | D-GN/WH | 1317 | Fog Lamp Relay Control (T96)
20 | YE | 5187 | Right Trailer Turn Signal Lamp (V92)
21 | OG | 5186 | Left Trailer Turn Signal Lamp (V92)
22 | PU | 709 | Left Park Lamp Supply Voltage
23 | PU | 92 | Windshield Wiper Motor High Speed
24 | D-GN | 95 | Windshield Wiper Motor Low Speed
25 | OG | 2268 | Windshield Washer Relay Control
26 | -- | -- | Not Used
27 | TN | 28 | Horn Relay Control
28 | PK | 1139 | Ignition 1 Voltage
29 | BN | 4 | Accessory Voltage
30 | PK | 1439 | Ignition 1 Voltage
31 | TN | 860 | Front Windshield Wiper Switch High Signal
32 | GY | 91 | Windshield Wiper Switch Signal 2
33 | RD/WH | 2540 | Battery Positive Voltage
34 | RD/WH | 2640 | Battery Positive Voltage (C69)
35 | RD/WH | 2740 | Battery Positive Voltage
36 | YE | 243 | Accessory Voltage
YE | 243 | Accessory Voltage
37 | -- | -- | Not Used
38 | PU | 544 | Headlamp Low Beam Supply Voltage
39 | WH | 17 | Stop Lamp Switch Signal
40 | WH | 1310 | EVAP Canister Vent Solenoid Control
41 | TN | 2759 | Low Reference
TN | 2759 | Low Reference
42 | BN/WH | 419 | MIL Control
43 | RD/BK | 242 | Battery Positive Voltage
44 | RD/BK | 442 | Battery Positive Voltage
45 | -- | -- | Not Used
46 | RD/BK | 842 | Battery Positive Voltage
47 | RD/BK | 642 | Battery Positive Voltage
A | RD/WH | 2540 | Battery Positive Voltage
B | L-GN | 2270 | Rear Window Washer Relay Control
C | RD/BK | 142 | Battery Positive Voltage

### Fuse Block - Underhood C3

#### Connector Part Information

- OEM: 6098-4937
- Service: See Catalog
- Description: 22-Way F Connector Assembly

#### Terminal Part Information

- Pins: 1, 2, 12, 22
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 3, 4, 4, 5, 6, 8, 9, 13, 14, 15, 16, 19, 20, 21, 7, 17, 18
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins 3, 4, 4, 5, 6, 8, 9, 13, 14, 15, 16, 19, 20, 21 - E/A
- Core/Insulation Crimp: Pins 7, 17, 18 - 2/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Fuse Block - Underhood C3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 409 | Cooling Fan Motor Supply Voltage
2 | BK | 1250 | Ground
3 | L-BU/WH | 1314 | Left Front Turn Signal Lamp Supply Voltage
4 | PU | 34 | Front Fog Lamp Supply Voltage (T96)
PU | 34 | Front Fog Lamp Supply Voltage (T96)
5 | D-BU/WH | 1315 | Right Front Turn Signal Lamp Supply Voltage
6 | BN/WH | 309 | Right Park Lamp Supply Voltage
7 | D-GN | 29 | Horn Control
8 | YE | 712 | Left Headlamp Low Beam Supply Voltage
9 | GY | 589 | DRL Resistor Supply Voltage
10-11 | -- | -- | Not Used
12 | GY | 532 | Cooling Fan Motor Supply Voltage
13 | PK/BK | 109 | Hood Ajar Switch Signal (AP3)
14 | PU | 5531 | Hood Closed Switch Signal (AP3)
15 | GY | 589 | DRL Resistor Supply Voltage
16 | PU | 709 | Left Park Lamp Supply Voltage
17 | D-GN | 392 | Rear Window Washer Pump Control
18 | D-BU | 298 | Rear Window Washer Pump Control
19 | TN/WH | 312 | Right Headlamp Low Beam Supply Voltage
20 | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage
21 | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage
22 | WH | 504 | Cooling Fan Low Reference

### Fuse Block - I/P C1

#### Connector Part Information

- OEM: 6098-5228
- Service: 88988709
- Description: 47-Way F LIF Series (GY)

#### Terminal Part Information

- Pins: 46
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 3, 13, 13, 14, 24, 25
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins 3, 13, 13 - E/A
- Core/Insulation Crimp: Pins 14, 24, 25 - 2/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 4, 5, 6, 8, 9, 15, 16, 18, 19, 20, 21, 21, 27, 28, 28, 28, 28, 29, 37, 39, 7, 32, 38
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins 4, 5, 6, 8, 9, 15, 16, 18, 19, 20, 21, 21, 27, 28, 28, 28, 28, 29, 37, 39 - E/C
- Core/Insulation Crimp: Pins 7, 32, 38 - C/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuse Block - I/P C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | RD/WH | 1640 | Battery Positive Voltage
4 | PK | 1139 | Ignition 1 Voltage
5 | RD/WH | 3340 | Battery Positive Voltage
6 | L-BU | 5986 | Serial Data Communication Enable
7 | OG | 1732 | Courtesy Lamps Supply Voltage
8 | PU/WH | 1382 | LED Dimming Signal
9 | PU/WH | 7005 | LED Dimming Signal (K34)
10-12 | -- | -- | Not Used
13 | RD/WH | 2340 | Battery Positive Voltage (UUC)
14 | RD/WH | 1040 | Battery Positive Voltage
15 | PK | 1139 | Ignition 1 Voltage
16 | TN | 28 | Horn Relay Control
17 | -- | -- | Not Used
18 | L-GN | 2270 | Rear Window Washer Relay Control
19 | RD/WH | 1040 | Battery Positive Voltage
20 | GY | 391 | Rear Window Wiper Switch Signal
21 | RD/WH | 1840 | Battery Positive Voltage
RD/WH | 1840 | Battery Positive Voltage
22-23 | -- | -- | Not Used
24 | RD/WH | 2040 | Battery Positive Voltage
25 | BK | 1450 | Ground
26 | -- | -- | Not Used
27 | PK | 1139 | Ignition 1 Voltage
28 | YE | 343 | Accessory Voltage (UUC)
29 | RD/WH | 840 | Battery Positive Voltage
30-31 | -- | -- | Not Used
32 | RD/WH | 1240 | Battery Positive Voltage
33-36 | -- | -- | Not Used
37 | D-GN | 5060 | Low Speed GMLAN Serial Data
38 | RD/WH | 240 | Battery Positive Voltage
39 | WH | 193 | Rear Defog Relay Control
40-45 | -- | -- | Not Used
46 | RD/BK | 442 | Battery Positive Voltage
47 | -- | -- | Not Used

### Fuse Block - I/P C2

#### Connector Part Information

- OEM: 7283-5600-40
- Service: See Catalog
- Description: 6-Way F (L-GY)

#### Terminal Part Information

- Pins: 4, 4
- Terminal/Tray: 7116-4121-02/10
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 1, 3, 2
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: Pins 1, 3 - D/G
- Core/Insulation Crimp: Pins 2 - A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Fuse Block - I/P C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/BK | 642 | Battery Positive Voltage
2 | RD/BK | 442 | Battery Positive Voltage
3 | RD/BK | 842 | Battery Positive Voltage
4 | RD/BK | 542 | Battery Positive Voltage (AG1)
5-6 | -- | -- | Not Used

### Fuse Block - I/P C3

#### Connector Part Information

- OEM: 6098-5229
- Service: 88988710
- Description: 50-Way F LIF Series (BK)

#### Terminal Part Information

- Pins: 1, 1, 34, 34
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 43, 44, 46, 47, C
- Terminal/Tray: 7116-4121-02/10
- Core/Insulation Crimp: C/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 45
- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: D/G
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

- Pins: 2, 3, 11, 12, 13, 23, 24, 35, A, 14, 14, 22, B, B
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins 2, 3, 11, 12, 13, 23, 24, 35, A - 2/A
- Core/Insulation Crimp: Pins 14, 14, 22, B, B - E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 4, 6, 6, 8, 9, 15, 18, 19, 20, 21, 27, 28, 29, 31, 32, 36, 37, 38, 41, 42, 5, 16, 16, 30, 39, 40
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins 4, 6, 6, 8, 9, 15, 18, 19, 20, 21, 27, 28, 29, 31, 32, 36, 37, 38, 41, 42 - E/C
- Core/Insulation Crimp: Pins 5, 16, 16, 30, 39, 40 - C/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fuse Block - I/P C3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN | 294 | Door Lock Actuator Unlock Control
TN | 294 | Door Lock Actuator Unlock Control
2 | TN | 294 | Door Lock Actuator Unlock Control
3 | TN | 694 | Driver Door Lock Actuator Unlock Control
4 | TN | 707 | RAP Relay Coil Supply Voltage
5 | L-BU | 1320 | CHMSL Supply Voltage
6 | L-BU | 1320 | CHMSL Supply Voltage
L-BU | 1320 | CHMSL Supply Voltage
7 | -- | -- | Not Used
8 | YE | 356 | Driver Door Lock Relay Unlock Control
9 | YE | 5704 | Endgate Latch Relay Coil Control
10 | -- | -- | Not Used
11 | RD/WH | 2140 | Battery Positive Voltage
12 | GY | 295 | Door Lock Actuator Lock Control
13 | YE | 643 | Accessory Voltage
14 | RD/WH | 1340 | Battery Positive Voltage
RD/WH | 1340 | Battery Positive Voltage
15 | PK | 1139 | Ignition 1 Voltage
16 | D-GN | 5060 | Low Speed GMLAN Serial Data
D-GN | 5060 | Low Speed GMLAN Serial Data (U2K)
17 | -- | -- | Not Used
18 | L-GN | 2270 | Rear Window Washer Relay Control
19 | GY | 391 | Rear Window Wiper Switch Signal
20 | D-GN | 5706 | Endgate Latch Relay Supply Voltage
21 | RD/WH | 2340 | Battery Positive Voltage
22 | L-BU | 6128 | Rear Closure Unlatch Motor Unlatch Control
23 | GY | 295 | Door Lock Actuator Lock Control
24 | RD/WH | 240 | Battery Positive Voltage
25-26 | -- | -- | Not Used
27 | TN | 28 | Horn Relay Control
28 | L-BU | 5986 | Serial Data Communication Enable
29 | L-GN | 2270 | Rear Window Washer Relay Control
30 | RD/WH | 440 | Battery Positive Voltage
31 | RD/WH | 2840 | Battery Positive Voltage
32 | RD/WH | 1840 | Battery Positive Voltage
33 | -- | -- | Not Used
34 | GY | 295 | Door Lock Actuator Lock Control
GY | 295 | Door Lock Actuator Lock Control
35 | RD/WH | 340 | Battery Positive Voltage
36 | PK | 1139 | Ignition 1 Voltage
37 | TN | 28 | Horn Relay Control
38 | L-BU | 5986 | Serial Data Communication Enable
39 | OG | 1732 | Courtesy Lamps Supply Voltage
40 | RD/WH | 1240 | Battery Positive Voltage
41 | L-BU | 5921 | Driver Door Unlock Relay Control
42 | L-GN | 1391 | Driver Door Unlock Relay Control
43 | RD/BK | 742 | Battery Positive Voltage
44 | YE | 143 | Accessory Voltage
45 | RD/BK | 242 | Battery Positive Voltage
46 | PU | 293 | Rear Defog Element Supply Voltage
47 | RD/WH | 2040 | Battery Positive Voltage
A | RD/WH | 640 | Battery Positive Voltage
B | RD/WH | 840 | Battery Positive Voltage (ASF, KA1)
RD/WH | 840 | Battery Positive Voltage (Except ATY , KA1)
C | YE | 143 | Accessory Voltage