For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the right instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement .
2. Remove the right console trim panel. Refer to Front Floor Console Side Trim Panel Replacement - Right Side .
3. Remove the instrument panel accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
4. Remove the instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement .

1 | Instrument Panel Lower Trim Panel Screw (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Lower Trim Panel Assembly
3 | Retainer Clip (Qty: 5)