For 1990-2009 cars

Important: Do not interchange the 30 mm torque converter housing bolts with the 28 mm fluid pump bolts.

1. Remove the 17 torque converter housing cover bolts/screws.
2. Remove the holding fixture bolt (1) to allow clearance for the housing.
3. Using a plastic hammer if needed, remove the torque converter housing assembly.
4. Install holding fixture bolt (1) after removal of the housing.