For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Camshaft Position Actuator

- Camshaft Bolt

58 N·m

43 lb ft

- Oil Control Valve Bolt

10 N·m

89 lb in

Camshaft Cap Bolt | 10 N·m | 89 lb in
Camshaft Cover Bolt | 10 N·m | 89 lb in
Camshaft Intermediate Drive Sprocket Bolt - Idler Sprocket | 58 N·m | 43 lb ft
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Connecting Rod Bolt

- First Pass

30 N·m

22 lb ft

- Second Pass - Counterclockwise

Back Off to Zero

- Third Pass

25 N·m

18 lb ft

- Final Pass

110 Degrees

Coolant Pipe Bolt | 10 N·m | 89 lb in
Crankshaft Balancer Bolt

- First Pass

100 N·m

74 lb ft

- Final Pass

150 Degrees

Crankshaft Main Bearing Bolt
Inner

- First Pass

20 N·m

15 lb ft

- Final Pass

80 Degrees

Outer

- First Pass

15 N·m

10 lb ft

- Final Pass

110 Degrees

Side

- First Pass

30 N·m

22 lb ft

- Final Pass

60 Degrees

Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position Sensor/Right Exhaust Manifold Lower Heat Shield

- Bolt

50 N·m

37 lb ft

Crankshaft Rear Oil Seal Housing Bolt | 10 N·m | 89 lb in
Cylinder Head Bolt - M8

- First Pass

15 N·m

11 lb ft

- Final Pass

75 Degrees

Cylinder Head Bolt - M11

- First Pass

30 N·m

22 lb ft

- Final Pass

150 Degrees

Cylinder Head Core Hole Plug | 75 N·m | 55 lb ft
Drive Belt

- Idler Pulley Bolt

50 N·m

37 lb ft

- Tensioner Bracket Bolt

23 N·m

17 lb ft

Engine Coolant Air Bleed Pipe Bracket Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 30 N·m | 22 lb ft
Engine Flywheel Bolt

- First Pass

30 N·m

22 lb ft

- Final Pass

45 Degrees

Engine Front Cover Bolt

- First Pass

20 N·m

14 lb ft

- Final Pass

60 Degrees

Engine Mount Bolt | 50 N·m | 37 lb ft
Engine Mount Bracket Bolt - Upper Right | 110 N·m | 81 lb ft
Engine Mount Bracket Bolts | 50 N·m | 37 lb ft
Engine Mount Bracket Nuts | 50 N·m | 37 lb ft
Engine Mount Strut Bolts | 25 N·m | 18 lb ft
Engine Mount Strut Bracket Bolts | 25 N·m | 18 lb ft
Engine Mount Strut Bracket Nuts | 110 N·m | 81 lb ft
Engine Mount Strut Nuts | 110 N·m | 81 lb ft
Engine Wiring Harness Bracket

- Bolt

25 N·m

18 lb ft

- Nut

13 N·m

115 lb in

Evaporative (EVAP) Purge Valve Bolt | 10 N·m | 89 lb in
Exhaust Manifold

- Bolt

25 N·m

18 lb ft

- Heat Shield Bolt

10 N·m

89 lb in

- Studs

10 N·m

89 lb in

Frame-to-Body Bolt | 155 N·m | 114 lb ft
Fuel Injector Sight Shield Cover Ball Stud | 10 N·m | 89 lb in
Fuel Rail Bolt | 25 N·m | 18 lb ft
Heater Inlet/Outlet Pipe Assembly Bolt | 10 N·m | 89 lb in
Ignition Coil Bolt | 10 N·m | 89 lb in
Intake Manifold

- Upper-to-Cylinder Head Bolt - Long

23 N·m

17 lb ft

- Upper-to-Cylinder Head Bolt - Short

23 N·m

17 lb ft

- Upper-to-Lower Intake Manifold Bolt

23 N·m

17 lb ft

Knock Sensor Bolt | 23 N·m | 17 lb ft
M14 Left Side Coolant Drain Threaded Plug | 31 N·m | 23 lb ft
Oil Drain Plug | 20 N·m | 15 lb ft
Oil Filter | 30 N·m | 22 lb ft
Oil Filter Fitting | 50 N·m | 37 lb ft
Oil Filter Housing Adapter Bolt | 23 N·m | 17 lb ft
Oil Gallery Plug | 31 N·m | 23 lb ft
Oil Level Indicator Tube Bolt | 10 N·m | 89 lb in
Oil Pan

- Bolt - Block M8

23 N·m

17 lb ft

- Bolt - Crankshaft Rear Oil Seal Housing M6

10 N·m

89 lb in

- Windage Tray Bolt

10 N·m

89 lb in

Oil Pressure Sensor | 20 N·m | 15 lb ft
Oil Pump

- Bolt

23 N·m

17 lb ft

- Cover Bolt

13 N·m

115 lb in

Oil Pump Suction Pipe Bolt | 10 N·m | 89 lb in
Piston Oil Cooling Nozzle Bolt | 10 N·m | 89 lb in
Primary Camshaft Drive Chain

- Left Lower Guide Bolt - Oil Pump - Second Design

23 N·m

17 lb ft

- Tensioner Bolt

23 N·m

17 lb ft

- Upper Guide Bolt

23 N·m

17 lb ft

Rear Engine Mount Bolts | 50 N·m | 37 lb ft
Secondary Camshaft Drive Chain

- Guide Bolt

23 N·m

17 lb ft

- Shoe Bolt

23 N·m

17 lb ft

- Tensioner Bolt

23 N·m

17 lb ft

Spark Plug | 20 N·m | 15 lb ft
Starter Motor Bolt | 50 N·m | 37 lb ft
Steering Intermediate Shaft Pinch Bolt | 34 N·m | 25 lb ft
Suction Tube Bolt | 10 N·m | 89 lb in
Suction Screen Bolt | 10 N·m | 89 lb in
Thermostat Housing Bolt | 10 N·m | 89 lb in
Throttle Body Bolt | 10 N·m | 89 lb in
Torque Converter Bolt | 60 N·m | 44 lb ft
Transmission

- Brace Bolt

50 N·m

37 lb ft

- To Engine Bolt

75 N·m

55 lb ft

Upper Intake Manifold Bolts | 25 N·m | 18 lb ft
Water Outlet Bolt | 10 N·m | 89 lb in
Water Pump

- Bolt

10 N·m

89 lb in

- Pulley Bolt

10 N·m

89 lb in

Wiring Harness Ground to Cylinder Head Bolt | 10 N·m | 89 lb in