For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Console Rear Bolt Cover (Qty: 2)

#### Procedure

1. Move the seat forward in order to access the rear bolt covers.
2. Use a flat-bladed plastic trim tool to remove the covers.

2 | Console Trim Plate Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
3 | Console Trim Plate Assembly - Rear

#### Procedure

1. Disconnect the electrical connections.
2. If replacing the console trim plate, transfer all necessary components.

4 | Retainer Clip (Qty: 1)