For 1990-2009 cars

### Removal Procedure

Caution: Refer to Glass and Sheet Metal Handling Caution in the Preface section.

1. Cover the mirror glass with tape.
2. Rotate mirror glass to expose the outer edge.
3. Insert a screwdriver or other flat-bladed tool 8.5 inches or longer and up to 0.4 inches wide into the slot between the mirror glass and mounting base as far as the tool will go.
4. Gently pull up on the tool and twist the tool until the glass releases off the base.
5. Remove the glass.
6. Disconnect the electrical connectors from the mirror if equipped with heated mirror.

### Installation Procedure

1. Connect the electrical connectors to the mirror if equipped with heated mirror.
2. Align the new mirror glass with the mounting base.
3. Install the mirror glass to the mirror motor with the palm of the hand on the center of the glass, pressing in until fully seated.
4. Inspect the mirror for proper operation.