For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Important: Apply Permatex® 24200 or equivalent on all seat belt fasteners prior to installation.
Center Rear Seat Belt Retractor-to-Seat Bolt | 45 N·m | 33 lb ft
Center Rear Seat Belt Retractor-to-Seat Nut | 45 N·m | 33 lb ft
Front Seat Belt Retractor Anchor Plate Bolt | 50 N·m | 37 lb ft
Front Seat Belt Buckle Bolt | 45 N·m | 33 lb ft
Front Seat Belt Height Adjuster Bolt | 40 N·m | 30 lb ft
Front Seat Belt Retractor Bolt | 45 N·m | 33 lb ft
Rear Seat Belt Buckle Bolt | 50 N·m | 37 lb ft
Rear Seat Belt Retractor Bolt | 45 N·m | 33 lb ft
Rear Seat Number 2 Belt Retractor Adjuster Bolt | 45 N·m | 33 lb ft
Rear Seat Number 2 Belt Retractor Bolt | 45 N·m | 33 lb ft
Rear Seat Number 2 Belt Retractor Anchor Bolt | 45 N·m | 33 lb ft
Seat Cushion Inner Finish Trim Panel Screw | 2 N·m | 18 lb in