For 1990-2009 cars

### Removal Procedure

1. Remove the rear door window regulator module. Refer to Rear Side Door Window Regulator Replacement .
2. Disconnect the outside handle rod from the latch.
3. Remove the outside handle bracket.
4. Disconnect the latch electrical connector.
5. Disconnect the latch arm from the window regulator module by depressing the tab and sliding rearward.
6. Disconnect the inside handle rod and lock button rod by twisting the latch.
7. Remove the latch from the latch arm by twisting.

### Installation Procedure

1. Install the latch to the latch arm by twisting.
2. Connect the inside handle rod and lock button rod by aligning the rods with clips and twisting the latch.
3. Connect the latch arm to the window regulator module by depressing the table and sliding rearward.
4. Connect the latch electrical connector.
5. Install the outside handle bracket.
6. Connect the outside handle rod to the latch.
7. Install the rear door window regulator module. Refer to Rear Side Door Window Regulator Replacement .