For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Steering Wheel and Column Description and Operation
2 | Verify the key cannot be removed from the ignition lock cylinder. Is the key stuck in the lock cylinder? | Go to Step 3 | System OK
3 | Is the vehicle equipped with a manual transmission? | Go to Step 6 | Go to Step 4
4 | Turn the ignition key to the OFF position. Can the key be turned to the OFF position and be removed? | Go to Step 6 | Go to Step 5
5 | Verify the adjustment of the range selector lever cable. Refer to Range Selector Lever Cable Adjustment . Can the key be turned to the OFF position? | System OK | Go to Step 6
6 | Inspect for a faulty lock cylinder. Is the lock cylinder damaged? | Go to Step 8 | --
7 | Inspect the ignition lock cylinder case. Is the case worn, damaged or loose? | Go to Step 9 | --
8 | Replace the ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement . Did you complete the repair? | Go to Step 10 | --
9 | Replace the ignition lock cylinder case housing. Refer to Ignition Lock Cylinder Case Replacement . Did you complete the repair? | Go to Step 10 | --
10 | Operate the system to verify the repair. Did you correct the condition? | System OK | Go to Step 2