For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Stabilizer Shaft Insulator Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Lower the rear suspension support. Refer to Support Replacement.

Tip
Lower the rear suspension support enough to remove the stabilizer shaft clamp bolt.

Tighten
70 N·m (52 lb ft)

2 | Stabilizer Shaft Insulator Clamp (Qty: 2)
3 | Stabilizer Shaft Insulator (Qty: 2)