For 1990-2009 cars

### Diagnostic Fault Information

Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

Circuit | Short to Ground | Open/High Resistance | Short to Voltage | Signal Performance
--- | --- | --- | --- | ---
Relay Switch B+ Circuit | 2 | 2 | -- | --
Rear Defogger Relay Control | B0283 02 | B0283 05 | B0283 05 | --
Rear Defogger Control Circuitt | 2 | 2 | 1 | --
Relay Coil Ground | -- | 2 | 2 | --
Rear Window Defogger Grid Ground | -- | 2 | 2 | --
1. Rear defogger always ON 2. Rear defogger Inoperative

### Circuit/System Description

When you depress the rear defogger button, voltage is supplied to the DEFOG relay coil and the HVAC control module also illuminates the rear window defogger indicator. Battery positive voltage is supplied at all times to the DEFOG relay switched input and the DEFOG relay coil is always grounded. This allows battery positive voltage from the relay switched input through the switch contacts and out the relay switched output to the rear window defogger. Ground for the rear defogger grid is provided by G401.

When you start the engine and press the rear defogger switch for the first time, the defogger cycle lasts for 15 minutes. Further operation results in 7.5 minute defogger cycles. The defogger cycle resets to 15 minutes when you cycle the ignition to the OFF position and then to the ON position.

### Reference Information

#### Schematic Reference

Defogger Schematics

#### Connector End View Reference

Window Systems Connector End Views

#### Description and Operation

Rear Window Defogger Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

• | Scan Tool Data List

• | Scan Tool Data Definitions

• | Scan Tool Output Controls

### Circuit/System Verification

1. Ignition ON, observe the operation of the Rear Defogger Grid while pressing the Rear Defogger Switch. The Rear Defogger Grid should ACTIVATE and DEACTIVATE when changing between commanded states.
2. Command the rear window defogger indicator ON and OFF with the scan tool. The rear window defogger indicator should turn ON and OFF when changing between the commanded states.

⇒ | If the Defogger Indicator does not illuminate, replace the HVAC control module.

### Circuit/System Testing

1. Ignition OFF, disconnect the REAR DEFOG relay.
2. Ignition OFF, test for less than 1.0 ohm of resistance between the relay coil ground circuit terminal 25 and ground.

⇒ | If greater than the specified range, test for an open/high resistance.

3. Ignition ON, verify that a test lamp does not illuminate between the relay controlled output circuit terminal 46 and ground.

⇒ | If the test lamp illuminates, test the control circuit for a short to voltage.

4. Verify that a test lamp illuminates between the relay switch B+ circuit terminal 43 and ground.

⇒ | If the test lamp does not illuminate, test the B+ circuit for a short to ground or an open/high resistance. If the circuit tests normal and the RR DEFOG circuit fuse is open, test the relay controlled output circuit terminal 46 for a short to ground

5. Ignition OFF, disconnect the harness connectors C1 and C2 at the Rear Defogger Grid.
6. Ignition OFF, test for less than 1.0 ohm of resistance between the Rear Defogger Grid ground circuit terminal 1 and ground.

⇒ | If greater than the specified range, test the ground circuit for an open/high resistance.

7. Connect the harness connectors at the Rear Defogger Grid.
8. Ignition ON, connect a 30-A fused jumper wire between the relay switch B+ circuit terminal 43 and the relay controlled output circuit terminal 46. Verify the Rear Defogger Grid is activated.

⇒ | If the Rear Defogger Grid does not activate, test the control circuit for an open/high resistance. If the circuit tests normal, test or replace the Rear Defogger Grid.

9. Connect a test lamp between the relay coil control circuit terminal 39 and the relay coil ground circuit terminal 25.
10. Command the Rear Defogger Grid ON and OFF by pressing the Rear Defogger Switch. The test lamp should turn ON and OFF when changing between the commanded states.

⇒ | If the test lamp is always ON, test the control circuit for a short to voltage. If the circuit tests normal, replace the HVAC Control Module.

⇒ | If the test lamp is always OFF, test the control circuit for a short to ground or an open/high resistance. If the circuit tests normal, replace the HVAC Control Module.

11. If all circuits test normal, test or replace the DEFOG Relay.

### Component Testing

#### Relay Test

1. Ignition OFF, disconnect the REAR DEFOG relay.
2. Test for 60-180 ohms of resistance between terminals 85 and 86.

⇒ | If the resistance is not within the specified range, replace the relay.

3. Test for infinite resistance between the following terminals:

• | 30 and 86

• | 30 and 87

• | 30 and 85

• | 85 and 87

⇒ | If not the specified value, replace the relay.

4. Install a 25-amp fused jumper wire between relay terminal 85 and 12 volts. Install a jumper wire between relay terminal 86 and ground. Test for less than 2 ohms of resistance between terminals 30 and 87.

⇒ | If greater than the specified range, replace the relay.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

• | Body Control Module Replacement

• | HVAC Module Assembly Replacement

• | Liftgate Window Replacement

• | Relay Replacement