For 1990-2009 cars

### Removal Procedure

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
2. Remove the surge tank inlet hose. Refer to Radiator Surge Tank Inlet Hose/Pipe Replacement.
3. Reposition the coolant air bleed hose clamp (1) at the coolant air bleed hose.
4. Remove the coolant air bleed pipe from the coolant air bleed hose (2).
5. Remove the coolant air bleed pipe bolts (3) from the upper intake manifold.
6. Remove the coolant air bleed pipe from the engine.

### Installation Procedure

1. Install the coolant air bleed pipe to the engine.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the coolant air bleed pipe bolts (3) to the upper intake manifold.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Install the coolant air bleed hose (2) to the coolant air bleed pipe.
4. Position the coolant air bleed hose clamp (1) at the coolant air bleed hose.
5. Install the surge tank inlet hose. Refer to Radiator Surge Tank Inlet Hose/Pipe Replacement.
6. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.