For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Place a drain pan under the oil pan drain plug.
3. Remove the oil pan drain plug (1). Allow the oil to drain completely.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the oil pan drain plug (1) and tighten to 20 N·m (15 lb ft.

Warning: Refer to Hot Exhaust System Warning in the Preface section.

5. Place the drain pan under the oil filter.
6. Remove the oil filter. Allow the oil to drain completely.

### Installation Procedure

1. Lubricate the NEW oil filter gasket with clean engine oil.
2. Tighten the oil filter to 30 N·m (22 lb ft).
3. Lower the vehicle.
4. Refill the engine oil. Refer to Approximate Fluid Capacities.
5. Start the engine and inspect for leaks.