For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment door assembly. Refer to Instrument Panel Compartment Door Replacement .

1 | Instrument Panel Compartment Screw (Qty: 9) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Compartment Assembly

#### Procedures

1. Disconnect the electrical connections.
2. When replacing the compartment assembly, transfer all the necessary components.