For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Bolt | 25 N·m | 18 lb ft
Air Cleaner Bolt | 10 N·m | 89 lb in
Air Cleaner Outlet Duct Clamp | 4 N·m | 35 lb in
Camshaft Position (CMP) Actuator Solenoid Valve Bolt | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 22 N·m | 16 lb ft
Evaporative Emission (EVAP) Canister Nut | 9 N·m | 80 lb in
Evaporative Emission (EVAP) Purge Solenoid Bracket Bolt | 10 N·m | 89 lb in
Fuel Fill Tube Clamp | 5 N·m | 44 lb in
Fuel Fill Tube Bracket Bolt | 9 N·m | 80 lb in
Fuel Rail Bolt | 10 N·m | 89 lb in
Fuel Tank Strap Bolt | 25 N·m | 18 lb ft
Heated Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Knock Sensor Bolt | 23 N·m | 17 lb ft
Left Rear Brake Line Fitting to Brake Crossover Pipe | 18 N·m | 13 lb ft
Mass Air Flow (MAF)/Intake Air Temperature Sensor Screw | 4 N·m | 35 lb in
Rear Exhaust Manifold Heat Shield Bolt | 50 N·m | 37 lb ft
Rear Brake Line to Rear Brake Hose Fitting | 18 N·m | 13 lb ft
Rear Brake Line Fitting to Brake Pressure Module | 21 N·m | 16 lb ft
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in