For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the driver side wheelhouse liner in order to access the washer container fasteners. Refer to Front Wheelhouse Liner Replacement.
2. Drain the washer solvent into clean container.
3. Remove the filler neck retainer from the radiator support.

1 | Windshield Washer Container Screws (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten Tighten the screws to 2.5 N·m (22 lb in)
2 | Windshield Washer Solvent Container Tip Ensure the grommet is attached to the bottom of the container upon re-assembly into the engine compartment.
3 | Windshield Washer Solvent Hose Tip Disconnect the washer solvent hose from the washer pump and container.