For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Wheelhouse Liner Replacement .

1 | Forward Lamp Wiring Harness Assembly
2 | Daytime Running Lamp Resistor Assembly Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 6 N·m (53 lb in)
3 | Daytime Running Lamp Resistor Assembly

#### Procedure

Disconnect the electrical connector.