For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Adjust the lumbar support knob until the lumbar basket is in the position of least support.
3. Remove the barrel end of the cable from the lumbar actuator.

1 | Front Seat Recliner Handle Tip Pull firmly forward on the handle to remove.
2 | Front Seat Outer Adjuster Finish Cover Refer to Front Seat Cushion Outer Trim Panel Replacement .
3 | Front Seat Belt Buckle Refer to Front Seat Belt Buckle Replacement .
4 | Front Seat Inner Adjuster Finish Panel Refer to Front Seat Cushion Inner Trim Panel Replacement .
5 | Front Seat Lumbar Support Actuator Knob Tip Remove the lumbar knob by pulling firmly on the knob.
6 | Front Seat Cushion Cover and Pad Refer to Front Seat Cushion Cover and Pad Replacement .
7 | Front Seat Lumbar Support Actuator Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
8 | Front Seat Lumbar Support Actuator