For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear seat. Refer to Rear Number 2 Seat Replacement .

1 | Rear Seat No. 2 Drive Link Cover Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear Seat No. 2 Drive Link and Cover
3 | Rear Seat Back Cushion Outer Support Cover Tip Pull outward to release from the seat frame.