For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Cargo Lamp Lens Tip Use a small flat bladed tool to aid in the removal of the lens.
2 | Cargo Lamp Assembly

#### Procedure

1. Using a small flat-bladed tool, disengage the cargo lamp attaching clips by gently prying at each side of the retaining tab while pulling the tab off of the headliner.
2. Pull the forward edge of the cargo lamp downward and rearward to disengage the lamp from the headliner.
3. Disconnect the electrical connector.