For 1990-2009 cars

### Removal Procedure

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front side water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Disconnect the electrical connector from the front side door window regulator motor.
4. Remove the front side window from the window regulator.

4.1. | Raise the window.

4.2. | Tape the window into position.

5. Remove the front side door window regulator motor screws.

### Installation Procedure

1. Align the front side door window regulator motor to the window regulator.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the front side door window regulator motor to regulator bolts .

Tighten the front door window regulator motor to door bolts to 8 N·m (71 lb in) .

3. Connect the electrical connector to the front side door window regulator motor.
4. Install the front side door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .