For 1990-2009 cars

### Removal Procedure

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Remove the front floor console. Refer to Console Replacement .
3. With park brake lever in the released position, using ONLY hand tools, remove the park brake cable adjusting nut and washer.
4. Release the rear park brake cable ends from the cable equalizer on the front cable.
5. Remove the front park brake cable from the park brake lever by pulling the cable rearward.

### Installation Procedure

1. Install the front park brake cable to the park brake lever.
2. Install the rear cable ends to the cable equalizer.
3. Using ONLY hand tools, install the washer and NEW adjusting nut (1) to the front park brake cable.
4. Adjust the park brake cable tension. Refer to Park Brake Adjustment .
5. Install the front floor console. Refer to Console Replacement .
6. Enable the SIR system. Refer to SIR Disabling and Enabling .