For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Remove the front door check link. Refer to Front Side Door Check Link Replacement .

1 | Front Side Door Upper Hinge Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove the water deflector.
2. Support the door before removing the hinge bolts.
3. Disconnect the electrical connector.
4. With the aid of an assistant, remove the door.

Tighten
31 N·m (23 lb ft)

2 | Front Side Door Lower Hinge Bolt (Qty: 2) Tighten 31 N·m (23 lb ft)
3 | Front Side Door Assembly

#### Procedure

When replacing the door it is necessary to transfer all of the internal components.