For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Brake Fluid Irritant Caution in the Preface section.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation .

1 | Brake Hose Fitting Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 52 N·m (38 lb ft)
2 | Brake Hose Fitting Gasket (Qty: 2) Tip DO NOT reuse the brake hose fitting gaskets. Install NEW gaskets.
3 | Brake Hose Bolt Tighten 12 N·m (106 lb in)
4 | Brake Hose Bracket Bolt Tighten 12 N·m (106 lb in)
5 | Brake Pipe Fitting Tip

• | Use a backup wrench when removing or installing brake pipe fittings.

• | Cap or plug the brake pipe fitting to prevent brake fluid leaks and contamination.

Tighten
18 N·m (13 lb ft)

6 | Brake Hose Tip Bleed the hydraulic brake system. Refer to Hydraulic Brake System Bleeding .